\section{(Adaptive Quadrature)}
Attached is the table generated by the MATLAB "tabulate" procedure for
both problems.  The safety factor was set to sigma = 0.9.  The results
are as to be expected: as the tolerance value $\tau$ decreases, the
accuracy increases; the number of function evaluations increases; the
largest and smallest step size accepted decrease.