NB: /usr/local/test/bin/{gcc,g++} are gcc-3.x snapshots; other gcc,
    g++ versions are 2.95.3
========================================================================
Apple PowerMac G3 (267 MHz);    GNU/Linux 2.2.18-4hpmac
/usr/bin/cc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (267 MHz);    GNU/Linux 2.2.18-4hpmac
/usr/bin/c++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (267 MHz);    GNU/Linux 2.2.18-4hpmac
/usr/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (267 MHz);    GNU/Linux 2.2.18-4hpmac
/usr/bin/g++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (267 MHz);    GNU/Linux 2.2.18-4hpmac
/usr/local/test/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (267 MHz);    GNU/Linux 2.2.18-4hpmac
/usr/local/test/bin/g++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (266 MHz);    GNU/Linux 2.4.10-12a
/usr/bin/cc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (266 MHz);    GNU/Linux 2.4.10-12a
/usr/bin/c++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (266 MHz);    GNU/Linux 2.4.10-12a
/usr/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (266 MHz);    GNU/Linux 2.4.10-12a
/usr/bin/g++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (266 MHz);    GNU/Linux 2.4.10-12a
/usr/local/test/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple PowerMac G3 (266 MHz);    GNU/Linux 2.4.10-12a
/usr/local/test/bin/g++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple Power Macintosh (233 MHz);                GNU/Linux 2.2.15pre9
/usr/bin/cc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple Power Macintosh (233 MHz);                GNU/Linux 2.2.15pre9
/home/beebe/ppc/local/bin/c++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple Power Macintosh (233 MHz);                GNU/Linux 2.2.15pre9
/home/beebe/ppc/local/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Apple Power Macintosh (233 MHz);                GNU/Linux 2.2.15pre9
/home/beebe/ppc/local/bin/g++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/ccs/bin/c89 -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/ucb/cc -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/ccs/bin/cc -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/local/bin/CC -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/ucb/cxx -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/local/bin/c++ -mieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/local/bin/gcc -mieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/local/bin/g++ -mieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/local/test/bin/gcc -mieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alpha 4100-5/266 (4 CPUs, 466 MHz, 2GB RAM);          OSF/1 4.0F
/usr/local/test/bin/g++ -mieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
Compaq AlphaServer DS20 Sierra/667 (EV?? 21264 CPU, 667 MHz, ????MB RAM); OSF/1 5.0
/usr/bin/c89 -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
Compaq AlphaServer DS20 Sierra/667 (EV?? 21264 CPU, 667 MHz, ????MB RAM); OSF/1 5.0
/usr/ucb/cc -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
Compaq AlphaServer DS20 Sierra/667 (EV?? 21264 CPU, 667 MHz, ????MB RAM); OSF/1 5.0
/usr/bin/cc -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
Compaq AlphaServer DS20 Sierra/667 (EV?? 21264 CPU, 667 MHz, ????MB RAM); OSF/1 5.0
/usr/bin/cxx -x cxx -ieee rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0xffc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
DEC Alphastation 200 4/100 (1 CPU, 100 MHz Alpha 21064 EV4, 64MB RAM);    GNU/Linux 2.2.19-6.2.1
/usr/bin/cc -ieee rwinfnan2.c
Floating exception (core dumped)
========================================================================
DEC Alphastation 200 4/100 (1 CPU, 100 MHz Alpha 21064 EV4, 64MB RAM);    GNU/Linux 2.2.19-6.2.1
/usr/local/bin/c++ -mieee rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
DEC Alphastation 200 4/100 (1 CPU, 100 MHz Alpha 21064 EV4, 64MB RAM);    GNU/Linux 2.2.19-6.2.1
/usr/local/bin/gcc -mieee rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
DEC Alphastation 200 4/100 (1 CPU, 100 MHz Alpha 21064 EV4, 64MB RAM);    GNU/Linux 2.2.19-6.2.1
/usr/local/bin/g++ -mieee rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
DEC Alphastation 200 4/100 (1 CPU, 100 MHz Alpha 21064 EV4, 64MB RAM);    GNU/Linux 2.2.19-6.2.1
/usr/local/test/bin/gcc -mieee rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
DEC Alphastation 200 4/100 (1 CPU, 100 MHz Alpha 21064 EV4, 64MB RAM);    GNU/Linux 2.2.19-6.2.1
/usr/local/test/bin/g++ -mieee rwinfnan2.c
Segmentation fault (core dumped)
========================================================================
HP 9000/712 (80 MHz PA-RISC 1.1 7100LC);  HP-UX 10.20
/usr/bin/cc rwinfnan2.c
NaN was written as: ?
Inf was written as: ++
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
HP 9000/712 (80 MHz PA-RISC 1.1 7100LC);  HP-UX 10.20
/home/beebe/bin/gcc rwinfnan2.c
NaN was written as: ?
Inf was written as: ++
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
IBM RS6000 43P-132 (133 MHz);  AIX 4.2
/usr/bin/cc rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM RS6000 43P-132 (133 MHz);  AIX 4.2
/usr/local/bin/CC rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM RS6000 43P-132 (133 MHz);  AIX 4.2
/usr/local/bin/c++ rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM RS6000 43P-132 (133 MHz);  AIX 4.2
/usr/bin/xlc rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM RS6000 43P-132 (133 MHz);  AIX 4.2
/usr/bin/xlC rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM RS6000 43P-132 (133 MHz);  AIX 4.2
/usr/local/bin/gcc rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM RS6000 43P-132 (133 MHz);  AIX 4.2
/usr/local/bin/g++ rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM SP2 (166 MHz);  AIX 4.3.2.0
/usr/vacpp/bin/c89 rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM SP2 (166 MHz);  AIX 4.3.2.0
/usr/vacpp/bin/cc rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM SP2 (166 MHz);  AIX 4.3.2.0
/uufs/inscc.utah.edu/common/home/mthnhb/ppc/local/bin/c++ rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM SP2 (166 MHz);  AIX 4.3.2.0
/usr/vacpp/bin/xlc rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM SP2 (166 MHz);  AIX 4.3.2.0
/usr/vacpp/bin/xlC rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM SP2 (166 MHz);  AIX 4.3.2.0
/uufs/inscc.utah.edu/common/home/mthnhb/ppc/local/bin/gcc rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
IBM SP2 (166 MHz);  AIX 4.3.2.0
/uufs/inscc.utah.edu/common/home/mthnhb/ppc/local/bin/g++ rwinfnan2.c
NaN was written as: NaNQ
Inf was written as: INF
NaN was correctly input as   0x7fc00000 NaNQ
Inf was correctly input as   0x7f800000 INF
========================================================================
Intel Pentium III (600 MHz);    GNU/Linux 2.2.17-14smp (Red Hat 6.2)
/usr/bin/cc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0xffc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Intel Pentium III (600 MHz);    GNU/Linux 2.2.17-14smp (Red Hat 6.2)
/usr/local/bin/c++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0xffc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Intel Pentium III (600 MHz);    GNU/Linux 2.2.17-14smp (Red Hat 6.2)
/usr/local/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0xffc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Intel Pentium III (600 MHz);    GNU/Linux 2.2.17-14smp (Red Hat 6.2)
/usr/local/bin/g++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0xffc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Intel Pentium III (600 MHz);    GNU/Linux 2.2.17-14smp (Red Hat 6.2)
/usr/local/sys/pgi/linux86/bin/pgcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was INCORRECTLY input as 0xffc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Intel Pentium III (600 MHz);    GNU/Linux 2.2.17-14smp (Red Hat 6.2)
/usr/local/sys/pgi/linux86/bin/pgCC rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was INCORRECTLY input as 0xffc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Intel Pentium III (600 MHz);    GNU/Linux 2.2.17-14smp (Red Hat 6.2)
/usr/local/test/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0xffc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Intel Pentium III (600 MHz);    GNU/Linux 2.2.17-14smp (Red Hat 6.2)
/usr/local/test/bin/g++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0xffc00000 nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Intel Pentium II (2 CPUs, 450 MHz);       FreeBSD 4.2.0
/usr/bin/c89 rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
Intel Pentium II (2 CPUs, 450 MHz);       FreeBSD 4.2.0
/usr/bin/cc rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
Intel Pentium II (2 CPUs, 450 MHz);       FreeBSD 4.2.0
/usr/bin/CC rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
Intel Pentium II (2 CPUs, 450 MHz);       FreeBSD 4.2.0
/home/staff/computing/beebe/i386/local/bin/c++ rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
Intel Pentium II (2 CPUs, 450 MHz);       FreeBSD 4.2.0
/home/staff/computing/beebe/i386/local/bin/gcc rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
Intel Pentium II (2 CPUs, 450 MHz);       FreeBSD 4.2.0
/home/staff/computing/beebe/i386/local/bin/g++ rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
SGI Origin/200-4;              IRIX 6.5
/usr/bin/c89 rwinfnan2.c
NaN was written as: nan0x7ffffe00
Inf was written as: inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
SGI Origin/200-4;              IRIX 6.5
/usr/bin/cc rwinfnan2.c
NaN was written as: nan0x7ffffe00
Inf was written as: inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
SGI Origin/200-4;              IRIX 6.5
/usr/bin/CC rwinfnan2.c
NaN was written as: nan0x7ffffe00
Inf was written as: inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
SGI Origin/200-4;              IRIX 6.5
/usr/local/bin/c++ rwinfnan2.c
NaN was written as: nan0x7ffffe00
Inf was written as: inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
SGI Origin/200-4;              IRIX 6.5
/usr/local/bin/gcc rwinfnan2.c
NaN was written as: nan0x7ffffe00
Inf was written as: inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
SGI Origin/200-4;              IRIX 6.5
/usr/local/bin/g++ rwinfnan2.c
NaN was written as: nan0x7ffffe00
Inf was written as: inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
SGI Origin/200-4;              IRIX 6.5
/usr/bin/DCC rwinfnan2.c
NaN was written as: nan0x7ffffe00
Inf was written as: inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
SGI Origin/200-4;              IRIX 6.5
/usr/bin/NCC rwinfnan2.c
NaN was written as: nan0x7ffffe00
Inf was written as: inf
NaN was INCORRECTLY input as 0x00000000 0
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/opt/SUNWspro/bin/c89 rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was correctly input as   0x7fffffff NaN
Inf was correctly input as   0x7f800000 Inf
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/usr/ucb/cc rwinfnan2.c
NaN was written as: nan0xfffffe00
Inf was written as: inf
NaN was correctly input as   0x7fffffff nan0xfffffe00
Inf was INCORRECTLY input as 0x00000000 0
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/opt/SUNWspro/bin/cc rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was correctly input as   0x7fffffff NaN
Inf was correctly input as   0x7f800000 Inf
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/opt/SUNWspro/bin/CC rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was correctly input as   0x7fffffff NaN
Inf was correctly input as   0x7f800000 Inf
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/usr/local/bin/c++ rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was correctly input as   0x7fffffff NaN
Inf was correctly input as   0x7f800000 Inf
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/usr/local/bin/gcc rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was correctly input as   0x7fffffff NaN
Inf was correctly input as   0x7f800000 Inf
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/usr/local/bin/g++ rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was correctly input as   0x7fffffff NaN
Inf was correctly input as   0x7f800000 Inf
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/usr/local/test/bin/gcc rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was correctly input as   0x7fffffff NaN
Inf was correctly input as   0x7f800000 Inf
========================================================================
Sun Ultra Enterprise 5500;     Solaris 2.7
/usr/local/test/bin/g++ rwinfnan2.c
NaN was written as: NaN
Inf was written as: Inf
NaN was correctly input as   0x7fffffff NaN
Inf was correctly input as   0x7f800000 Inf
========================================================================
Sun SPARC 10/51;               GNU/Linux 2.2.19-6.2.1 (Red Hat 6.2)
/usr/bin/cc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fffffff nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Sun SPARC 10/51;               GNU/Linux 2.2.19-6.2.1 (Red Hat 6.2)
/usr/local/bin/c++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fffffff nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Sun SPARC 10/51;               GNU/Linux 2.2.19-6.2.1 (Red Hat 6.2)
/usr/local/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fffffff nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Sun SPARC 10/51;               GNU/Linux 2.2.19-6.2.1 (Red Hat 6.2)
/usr/local/bin/g++ rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fffffff nan
Inf was correctly input as   0x7f800000 inf
========================================================================
Sun SPARC 10/51;               GNU/Linux 2.2.19-6.2.1 (Red Hat 6.2)
/usr/local/test/bin/gcc rwinfnan2.c
NaN was written as: nan
Inf was written as: inf
NaN was correctly input as   0x7fffffff nan
Inf was correctly input as   0x7f800000 inf
